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Proposed Validation list to be used by LPAS, prior to consultation
	Item 
	Description
	APPLICANT TO COMPLETE 
Document Reference and page number
	LPA to check if it has been submitted (Yes/No)


	1
	Site Surveys (if appropriate)
	
	

	
	Topographic survey 
	Survey Solutions Ltd drawing no. 65958BWLS-01
	

	
	Details of existing site layout, drainage, and catchment areas plus pre and post development impermeable areas
	N/A
	

	
	Evidence of % increase for urban creep and how it’s been applied to post development calculations
	Appendix D of FRA - JPP Consulting Ltd (report ref. R-FRA-28236-01-E).

JPP Consulting File ref. 28961 – Harpenden SW Drainage Calculations
	

	
	Ground investigation including groundwater level information (for seasonally high groundwater level), potential contamination and infiltration testing (to BRE365 or similar)
	Ground investigation: RPS Group report ref. 794-DES-CAS-31270
Pages 3 – 5, 11
Soakage testing: Southern Testing Environmental & Geotechnical Project ID: JN1933-PERM
	

	
	Existing drainage scheme survey e.g., CCTV or historic plans
	N/A
	

	
	Survey of existing waterbodies e.g., watercourses, ponds or springs and culverts or bridges
	N/A
	



	2
	Plans and Drawings
	
	

	
	Layout drawing including drainage scheme SuDS and other water features.  Including invert levels, cover levels, conveyance systems any pipe gradients, flow directions and labels that match any drainage modelling calculations.  Outfall locations, control devices, attenuation systems and water quality treatment features. 
	Section 5.9 and Appendix D of FRA - JPP Consulting Ltd (report ref. R-FRA-28236-01-E).
Page 28
	

	
	[bookmark: _Hlk221270793]High level construction management plan including phasing access arrangements and operational characteristics.  Temporary drainage and water pollution including discharge points and flow controls should be included.
	Construction drainage to be in line with SuDS manual Chapter 31. Appointed contractor to provide upon appointment.

	

	
	[bookmark: _Hlk221270804]Landscaping planting scheme for vegetated SuDS
	N/A - Detailed planting will come through as part of future Reserved Matters
	

	
	Maintenance plan and confirmation in principle of adopting authority for the lifetime of the development
	Section 7.0 of FRA - JPP Consulting Ltd (report ref. R-FRA-28236-01-E).
Pages 30 – 34
	

	3
	Assessments
	
	

	
	Evidence that that the SuDS hierarchy and the 4 pillars have been met.
	Sections 5.3, 5.5 and 5.6 of FRA - JPP Consulting Ltd (report ref. R-FRA-28236-01-E).
Pages 23 – 27

	

	
	Full supporting calculations for the drainage design including design parameters using FEH 13 and predevelopment greenfield runoff rates / volumes. 
	JPP Consulting File ref. 28961 – Harpenden SW Drainage Calculations
	




	
	Critical storm simulation results of the conveyance network by level and discharge for events 100%, 3.33%,3.33% plus climate change, 1% and 1% AEP plus climate change 
	JPP Consulting File ref. 28961 – Harpenden SW Drainage Calculations
	

	
	Evidence of calculations to support the sizing of storage features to accommodate the 3.33% AEP plus climate change and 1% AEP climate change critical storms.
	JPP Consulting File ref. 28961 – Harpenden SW Drainage Calculations
	

	
	Evidence and drawing of where any flooding would occur during a 1% AEP plus climate change critical storm event would occur.  Information should include extent, depth, and velocity of flooding, demonstrating that it would not leave the site boundary.
	JPP Consulting File ref. 28961 – Harpenden SW Drainage Calculations
	

	
	Flood resistance and resilience measures 300mm above flood levels
	N/A
	

	
	Drawing showing exceedance flows greater than 1% AEP plus climate change or if the drainage system is compromised.
	JPP Consulting File ref. 28961 – Harpenden SW Drainage Calculations
	

	4
	Supplementary Evidence
	
	

	
	Confirmation of discharge location approval (in principal agreements from third parties if appropriate)
	Sections 5.3 of FRA - JPP Consulting Ltd (report ref. R-FRA-28236-01-E).
Pages 23 – 24
Sections 6.0 of FRA - JPP Consulting Ltd (report ref. R-FRA-28236-01-E).
Page 29

	

	
	Confirmation of any consents required
	N/A. Surface water to be managed via infiltration within the development.
	

	
	Evidence of predevelopment discharge capacity analysis (where discharging from an existing pipe).
	Sections 6.0 and Appendix E of FRA - JPP Consulting Ltd (report ref. R-FRA-28236-01-E).
Page 29
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